{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Nabava autobusne nadstrešnice"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Nabava autobusne nadstrešnice","index":0,"n_rows":13,"n_cols":6,"rows_kept":13,"cut":false,"hidden":false,"merged":[[2,0,3,5],[7,0,9,0],[7,1,9,1],[7,2,9,2],[7,3,9,3],[7,4,9,4],[7,5,9,5]]}
[null,"Prilog 2. "]
[]
["PREDMET: TROŠKOVNIK  -  Nabava i ugradnja autobusnih stajališta na području Grada Crikvenice; ev.br.: 41-03-26-JN"]
[]
[]
["R.B.","OPIS ","J.M.","KOL.","JEDINIČNA CIJENA € (bez PDV-a)","UKUPNA CIJENA U € (bez PDV-a)"]
[null,"Lokacija: Dramalj, Manestri i Dramalj, Milovana Muževića"]
["1.","Dobava, doprema i montaža autobusne nadstrešnice, dimenzija d 4900 x š 1200 (krov) x v 2370 mm (± 5mm); kontrukcija inox;  noga nadstrešnice (4 kom) sastavljena iz dvije cijevi promjera 48,3 mm (± 1mm), međusobno spojene pločicama na pet mjesta, dva žlijeba rš.500mm (± 1mm), dužina žlijeba je dužina nadstrešnice uvećana za 300 mm(± 1mm) s obje strane; lučni nosači izvedeni iz cijevi 60/40 mm (± 1mm),  pokrov: krovni akrilat debljine min 4 mm, prozirni, učvršćen inox ili alu trakama; stakla kaljena 1345/2000/10 mm (± 1mm), kom 3; držači stakla inox kom 6 po staklu. Nadstrešnicu opremiti sa inox klupom s PVC letvicama dimenzija 1414 x 400 x 400 mm (± 5mm). ","kpl",2]
[]
[]
[null,null,null,null,"UKUPNO:"]
[null,null,null,null,"PDV 25%"]
[null,null,null,null,"SVEUKUPNO:"]